{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":7,"rows_kept":9,"merged":[[0,0,0,5],[1,2,1,6],[7,0,7,4],[8,0,8,4]],"flags":["formulas_cached_only"]}
["材料报价清单"]
["工程名称：","2022年商品粮大市奖励资金安州区金谷道粮食储备库升级改造项目\\单项工程1【建筑与装饰工程】",null,null,"","",""]
["序号","名称、规格、型号","单位","数量","投标单价(元)","合价（元）"]
[1,"瓦：规格450*300水泥彩瓦","m2",1050.21]
[2,"防水卷材：规格材质4厚SBS防水卷材，符合国家标准GB/T18242-2008","m2",1050.21]
[3,"硅钙板：规格10厚600*600硅钙板，符合国家标准GB/T 25975-2010《硅酸盐复合板材》","m2",934]
[4,"烧结砖：规格240*115*53，页岩砖，等级MU15","千匹",29.625]
["本页小计"]
["分部合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}